

Product Advisory

QTP Part Number 61288

Please be advised due to the paint priming process that there maybe a build of paint on the thread of the filler neck. We advise that this paint be cleaned off using a wire brush as this will allow smooth fitment of the cap. Thank you for taking the time to read this.

Before

A stack of plates on a table

Description automatically generated

After

A group of metal rings on a white surface

Description automatically generated